NEPOOL Operating Procedures
OP 10 – Analysis and Reporting of

Power System Emergencies


Appendix B – DOE & State Regulatory Agency Report Criteria


APPENDIX B

DOE AND STATE REGULATORY AGENCY REPORT CRITERIA

(See Section II.A for detail reporting criteria) 

(See APPENDIX C for DOE and State Agency Telephone Numbers)

REPORT CRITERIA
REPORT DEADLINES

1 a. Manual or Automatic Load Shedding of 100 MW or more (OP7)
As soon as practicable after event but within three (3) hours

1 b. Loss of service of more than 200 MW of firm loads for more than 15 minutes


1 c. Any continuous outage of more than 50,000 customers for three (3) hours or more


*2 a. Anticipated or Implemented Voltage Reductions (NEPOOL OP NO. 4 - ACTIONS 12 and 13
As soon as practicable after event but within twenty-four (24) hours.

*2 b. Any request to reduce the use of bulk power supply electricity to maintain adequacy. (NEPOOL OP NO. 4 - ACTIONS 14 and 15)
 

3a .Any actual or suspected act(s) of physical sabotage (not vandalism) or terrorism directed at the bulk electric power supply system in an attempt to either disrupt degrade or deny service reliability
As soon as practicable after event but within twenty-four (24) hours.

3b.Other abnormal emergency system operating conditions or events that could constitute a hazard to maintaining the continuity of the bulk power supply system.
As soon as practicable after detection of the condition.

4.Fuel Emergency 
As soon as practicable but within three (3) days.

* The criteria listed above constitute the minimum reporting requirements.  Some states require reports when other Actions of OP NO. 4 are implemented.
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